BusinessPhone Communication Platform 6.0
Dialogs

## Least Cost Routing

Least Cost Routing is a feature that selects the most economic carrier for an entered destination number.

This dialog is used to define the general settings for Least Cost Routing (LCR), like the directory number for LCR, the dial tone initiating and a predicated call duration for the call cost calculation.

To access the dialog, open the “Facilities” menu in the Configuration directory tree and click on the “Least Cost Routing” submenu.

The following commands are available:

5623 |  | LCR directory number

2024 |  | Initiate public dial tone at LCR

2034 |  | Initiate dial tone at LCR

2035 |  | Predicated call duration

For more information about a setting or a field, click on the command link in brackets to open the online help system.

#### Actions

Submit |  | To apply the changed parameters in the programmable key dialog. |
Reload |  | To reload the current system settings. |

For more information on Least Cost Routing see facility description Least Cost Routing (321/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2004