BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2034
Initiate dial tone at LCR

This command defines whether or not a dial tone should be transmitted to the caller after dialling the directory number of a trunk which is controlled by LCR.

Y .... Initiate dial tone sending |  |

N .... Do not initiate dial tone sending |  |

See: Command 1026 LCR analysis required |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004