BusinessPhone Communication Platform 6.0
Dialogs

## ELU-D Line Error

This dialog is used to study the line error counters that had been initiated by an ELU-D card.

Note

You can access ELU-D only!:

Card |  | To select the card |
Card / Individual |  | To define the card and related individuals. |
Bit Violation |  | Maximum number of bit violation errors during one second. The bit violation is anaylized every 20 ms. If there is at least one bit fault since the last read-out, the counter is incremented by one. |
Messages lost |  | Number of sent messages that have been lost, i.e. if a message has not been acknowledged after three attempts. |
NAK transmitted |  | Number of NAK’s for transmitted messages. |
NAK received |  | Number of NAK’s for received messages |
Time-outs transmitted |  | Number of timeouts for transmitted messages, i.e. no answer from the connected device. |
Time-outs received |  | Number of timeouts for received messages, i.e. not completed in the time specified. |

#### Actions:

Submit |  | To submit all changes to the System. |
Clear |  | To clear the error counter of the card. The button is only displayed when a card is selected. |

Revision: B © Ericsson Enterprise 2004