BusinessPhone Communication Platform 6.0
Dialogs

## Transmission Test Control

### Level Adjust

This function allows control of the automatic transmission level adjustments in the connected system.

Current adjust mode: <actual mode> |  |

Change mode to Normal or Freeze |  |

#### Fields

Freeze: No further level adjustments are made. Levels remain at the current settings. |  |

Normal: Transmission levels are adjusted according to the connected parties. |  |

Note

Level adjustments are made when connections are setup. When you change from FREEZE to NORMAL the currently active connections are not affected.

### Silent Channel

This function is valid only for a connection that has already been established between two parties. It allows switching between the states SILENT and NORMAL for one of the parties.

For directory number: <directory number used for mode> |  |

Set mode to: Normal or Silent |  |

#### Fields

Silent: The transmission path to the selected directory number is the transmission path to the selected directory number is pcm pattern, which is received as 'silent' on analogue equipment. The transmission from the selected directory number is not affected. |  |

Normal: The normal two-way connection is restored. |  |

### Actions

Submit... Submit all changes to the System. |  |

Revision: B © Ericsson Enterprise 2004