BusinessPhone Communication Platform 6.0
Dialogs

## Queue Settings

This dialog allows to change settings for the queue dump and the load regulation queue.

### Queue Dump

The BusinessPhone operating system provides a mechanism for dumping the content of different message queues within the exchange to a specific memory area. This dumping process will be performed when the number of entries within a queue exceeds a certain threshold.

The threshold value for different queues within a BusinessPhone system can be defined in this dialog. You can select a different value for each queue.

#### Queue limits and default values:

Queue |  | Range |  | Default |
JQB |  | 16 - 113 |  | 16 |
JQC |  | 32 - 341 |  | 32 |
JQD |  | 64 - 453 |  | 64 |

The upper limit is calculated by assuming a message length of 6 bytes, while the lower limit assumes a maximum possible message length of 61 bytes. The number of messages that can be stored in a queue defines the available range.

Additionally, the time between two watchdog triggers can be set up within this menu in steps of 250 ms.

1 ... 250 ms

2 ... 500 ms

3 ... 750 ms

...

15 ... 3750 ms.

A default value of 8 or 2 s is established automatically.

#### Load Regulation Queue:

The operating system of ASB 15002 maintains a facility where, messages designated for job queue B are stored in an intermediate queue, to regulate the load on job queue B.

The Load Regulation Queue is mainly used by TR in case of simultaneous incoming calls, in order to prevent the operating system from running out of buffers. A maximum number of 80 messages can be stored at once in the Load Regulation Queue.

The time delay between two successive messages taken from the queue can be defined within this menu by steps of 250 ms.

A default value of 1 (250 ms) is set automatically.:

Enable Queue Dump |  | Enables / Disable the queue dump facility. |
Time between watchdog triggers |  | The time between two watchdog trigger time-outs. |
Threshold Job Queue B |  | Size of the queue B. |
Threshold Job Queue C |  | Size of the queue C. |
Threshold Job Queue D |  | Size of the queue D. |
Maximum number of queue entries |  | Maximum number of stored messages in the Load Regulation Queue. |
Time delay in load regulation queue |  | The time between two successive messages. |

#### Actions:

Submit |  | To submit your changes to the system. |
Reload |  | To reload the currently displayed data block. |

Revision: B © Ericsson Enterprise 2004