BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0x2B
Directory Number Error

Default definition: |  | ALARM + EXTERN + ACTIVE |
Used by block: |  | E2 |
Category: |  | MAINTENANCE |

Two identical directory numbers have been found during the start-up of the E2 data handler.

- D1: Directory number, high byte
- D2: Directory number, low byte
- D3: Undefined
- D4: Undefined

#### Recommended action

Use command 5901 to find out, to which function the directory number belongs to. Replace this directory number temporarily with a free (non-utilised) number. Then use the function ‘eeprom resources/test’. This will cause the internal directory number table of the exchange to be updated. See also warning code 2CH.

With command 5901 it is now possible to find out, which other function occupies the directory number in question. Make a definitive correction of the directory numbers for the two functions.

Revision: I © Ericsson Enterprise 2004