BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2198
H.323 Trunk GW Password

This command defines the own H.323 Trunk GW Password and is used for incoming calls. If BusinessPhone gets an incoming call then the received password is compared with 2198 H.323 Trunk GW Password (Own H.323 Trunk GW Password).

Incoming calls, which do not supply password will be accepted and processed only if the originator can be identified as one of preconfigured gateways (i.e. the calling party call signalling address must match the call signalling address of a preconfigured gateway - "1000 node" table - command 2164 Network IP address), all other call attempts will be rejected with the reason “securityDenied“.

##### Valid data

0-8 characters |
empty (default) |

Note

In case, that the calling PBX is a BusinessPhone, then the command 2187 Network Node Password of the calling BusinessPhone has to correspond with the value of command 2198 H.323 Trunk GW Password of the gateway of the called BusinessPhone.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004