BusinessPhone Communication Platform 6.0
Commands > Commands 9000...9999

## 9143
Predigits choice 4

This command is used to define predigits, if any, for the 4-th route choice. The predigits are transmitted after the private network access code and before the dialled external number.

Predigits = 1-16.

Following commands for the 2-nd route choice will be ignored:

3302 Call back allowed |  |

3303 Predigits |  |

3304 Alternative route choice 1 |  |

3305 Predigits choice 1 |  |

3306 Alternative route choice 2 |  |

3307 Predigits choice 2 |  |

##### Valid data

0-24 |  |  |
(blank) |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004