BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0168
Use ACD key layout

The command defines whether or not the ACD key layout shall be used on a DBC 2x1/2x2 or DBC 223 telephone.

##### Valid data

0 |  | business layout |
1 |  | ACD key layout with clerical key |
2 |  | ACD key layout without clerical key |

Note

If a DBC213 is changed against a DBC 223 watch out, that the ACD keys are not programmed twice.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004