BusinessPhone Communication Platform 6.0
Dialogs

## Application I/O

In this dialog, you can determine the line positions for communication channel 0 and 1, select the type of operation for calls and hotel data, define the data in the data record and configure many more settings.

To access the dialog, open the “Interfaces” menu in the Configuration directory tree and click on the “Application I/O” submenu.

The dialog consists of two parts:

- configuration of the application I/O
- test protocol I/O

The following commands are available for communication channel 0 and channel 1 and the test protocol settings:

6401 |  | Initiate I/O ports

6402 |  | Activate I/O ports?

6403 |  | Format table

6404 |  | Lines per page

6405 |  | I/O time supervision

6406 |  | Automatic I/O activation

6407 |  | CIL-data via CTI-link

6431 |  | Test protocol port address

6432 |  | Enable test protocol

For more information about a field or a setting, click on the respective command link in brackets.

#### Actions:

Submit |  | To submit your changes to the system. |
Reload |  | To reload the current system settings. |

For more information, see also System Description (1551-ASB 150 02 Uen) and facility description Computer Telephony Integration (CTI) (152/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2004