BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1109
Common announcement interruptable

This command states whether the alerting on the answering/reroute position shall start at the same time as the common trunk announcement and the announcement can be interrupted by answering the call or if the voice message shall be sent out completely before alerting starts.

##### Valid data

NO |  | Common announcement not interruptable |
YES |  | Common announcement interruptable |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004