BusinessPhone Communication Platform 6.0
Dialogs

## Operator

In this dialog, you can define the Operator settings.

To access the dialog, open the “Features” menu in the Configuration directory tree and click on “Operator”.

The following commands are available:

#### Directory Info

5613 |  | Directory number

6501 |  | Directory name

#### Operator functions

4001 |  | Alternative answer position

4003 |  | Answering time

4004 |  | Cyclical selection

4005 |  | Auto. answer superv. time

4006 |  | Queue announcement time

4007 |  | Queue announcement reference

4008 |  | Calling of extension at incoming call

4009 |  | Two external lines at operator 3-party

4010 |  | Two PE-lines at operator 3-party

4011 |  | Listening during the announcement

4012 |  | Sending a ready tone after announcement

#### Operator individuals

4101 |  | Operator line position

4102 |  | Operator answer reference

4103 |  | Ring burst at queue?

4104 |  | Receiving of tone signals

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To reload the current system settings. |

See facility description Operator (380/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2004