BusinessPhone Communication Platform 6.0
Commands > Commands 8000...8999

## 8733
Default exit position

When an external or internal party connected to a CTI Group (see command 5428 Create CTI Group) types a customer-id which is longer than 16 digits, an error announcement will be played (see command 4411 Command to record the new AA announcement group). If there is a second wrong response in the same menu level or resources are missing or the telephony server gives back an invalid directory number the caller will be rerouted to the directory number stated in this command.

If no reroute position is specified (DIR.NONUM) an external call will be rerouted to the reroute position of the incoming trunk. (see command 1103 Reroute position at day, 1104 Reroute position at night). An internal call will be disconnected.

##### Valid data

Decimal number |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2004