BusinessPhone Communication Platform 6.0
Commands > Commands 6000...6999

## 6014
Dialled number

The command determines the digits constituting the dialled number.

The following characters may be used:

##### Valid data

Valid values |  | 20 digits |
0-9 |  | Digit to be sent |
*, # |  | Character to be sent |
- |  | Wait for second dial tone |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004