BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0xAA
Invalid SP-Status

Default definition: |  | ERROR |
Used by block: |  | SP |
Category: |  | DESIGNER |

This code indicates an internal error in the SP program. The warning indicates, that an internal or external command is received in an invalid state.

- D1: Current state

- There are several state variables in SP. No exact definition is done.

- D2: Type of command

- F0h: Receiver interrupt
- F1h: Transmitter interrupt

- D3: Undefined
- D4: Undefined

Revision: I © Ericsson Enterprise 2004