BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1306
Inter digit pause

The command is used to determine the pause between the digits valid for decadic impulsing.

00 = |  | 300ms |  | 08 = |  | 700ms |
01 = |  | 350ms |  | 09 = |  | 750ms |
02 = |  | 400ms |  | 10 = |  | 800ms |
03 = |  | 450ms |  | 11 = |  | 850ms |
04 = |  | 500ms |  | 12 = |  | 900ms |
05 = |  | 550ms |  | 13 = |  | 950ms |
06 = |  | 600ms |  | 14 = |  | 1000ms |
07 = |  | 650ms |  | 15 = |  | 1050ms |

##### Valid data

00-15 |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004