BusinessPhone Communication Platform 6.0
Commands > Commands 5000...5999

## 5410
Create call number for standard paging

ASB 150 permits connection of external equipment for paging via radio or a magnetic loop. Connection is achieved via a trunk (external line) board that has been reserved for this purpose.

This command is used to create a function for standard paging. The stated directory number must be free and must not conflict with any existing directory number; it is used to set up paging. Standard paging means that paging takes place using the “meet-me” or “call-me” principle without the pager being able to transmit his/her own orders to the paging receiver.

Command 5411 Create call number for alternative paging is used to create a function for “alternative” paging and command 5412 Create answer number for meet-me is used to create a function for answer in accordance with the meet-me principle.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004