BusinessPhone Communication Platform 6.0
Commands > Commands 5000...5999

## 5301
Define authority level

This command allows the reading/changing of the authorization level at which a certain command is placed. Authorization level 0 is the lowest level in the system, i.e the operator on this level has lower authorization than operators on higher levels.

To be able to change the authorization level for a command, a special authorization check is required, see the table below:

Operator Authorization level | Command Authorization level
| 0 | 1 | 2 | 3
0 | - | - | - | -
1 | 1 | 0 | - | -
2 | 1,2 | 0,2 | 0,1 | -
3 | 1,2,3 | 0,2,3 | 0,1,3 | 0,1,2

The figures shown in the table indicate the authorization level/s to which may be changed. A-indicates that no change is permitted.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004