BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0xB8
MG Outcall Notification Error

Default definition: |  | MG OUTCALL NOTIFICATION ERROR |
Used by block: |  | MG |
Category: |  | MAINTENANCE |

Lowest MG warning level. An abnormal condition in the program and in the start-up has been detected by the MG program. The condition was safely handled by the software and does not require immediate user assistance.

- D1: Type of warning

- 01h ... Process creation error, resources not available.
- 02h ... User linked record (33) read error.
- 03h ... Notification request older than two days.
- 04h ... No free record to insert the notification request.
- 05h ... BBRAM error after successful start-up.
- 06h ... Message arrived to a not running prcess.
- 07h ... BBRAM error during start-up, OCN is blocked.

- Error situations during a notification attempt:

- 10h ... User linked record (33) read error.
- 11h ... User base record read error.
- 12h ... Directory number conversion.
- 13h ... Invalid external number.
- 14h ... User has no full or breaf notification setting.
- 15h ... Invalid SEIZNAK message from ST.MGINP.
- 16h ... TR released the SEIZCALL.
- 17h ... OCN received no SEIZLCR forward data.
- 18h ... No more digit to dial.
- 19h ... TR aborted the current notification with CONRELCTRL.
- 1Ah ... OCN has trieds the notification more than 256 times.

##### The following parameters are only valid , if D1 is higher than 0Fh.

- D2: OCN process state.
- D3: User directory number, high byte.
- D4: User directory number, low byte.

Revision: I © Ericsson Enterprise 2004