BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2096
COLR display handling

The command is used to state the type of COLR display handling:

- to display the dialled (called) number or
- to display the text “DISPLAY RESTRICTED” after received COLR from the public/private ISDN.

Note

In case that BusinessPhone does not receive the ISDN message “COLR”, BusinessPhone displays always the dialled (called) number.

##### Valid data

Value | Meaning | Display
1 | Public COLR | dialled number
2 | Public and Private /proprietary COLR | dialled number
3 default | Public and Private /proprietary COLR | DISPLAY RESTRICTED

Minimum required authority level from telephone: No

Accessible via BMS: Yes

For further details pls. refer to ISDN SS Connected Line Identification Restriction (COLR)

Revision: J © Ericsson Enterprise 2005