BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1307
PTS-signal from parent exchange?

The command is used to state whether the exchange shall wait for a proceed-to-send signal (PTS signal) from the parent exchange. See command 1404 Wait time before start to send digits when no PTS for wrong proceed-to-send signal if the exchange does not send any signal.

(Command 1308 PTS-signal from parent exchange = dial tone? states whether the proceed-to-send signal is the dial tone. See also command 1013 Dial tone to extension?, which states whether dial tone shall be sent to the extension.)

##### Valid data

No |  |  |
Yes |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005