BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2149
Suppress direct media routing

Defines whether direct media routing on IPUs should be suppressed.

##### Valid data

Yes |  | direct media routing suppressed - in this case MOH and call progress tones are sent to the IP-client independent on command 2180 MOH and call progress tones to H.323 clients |
No (default) |  | direct media routing not suppressed |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005