BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2176
Trusted H.323 Extension IP Address Range

This command defines up to 6 IP address ranges from which the Gatekeeper accepts registration requests from H.323 extensions.

##### Valid data

| low value | high value
Zone1-6 | 0.0.0.0 -255.255.255.255 | 0.0.0.0 -255.255.255.255
Zone1 (default) | 0.0.0.0 | 255.255.255.255
Zone 2-6 (default) | 0.0.0.0 | 0.0.0.0

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005