BusinessPhone Communication Platform 7.0
Maintenance Instruction ASB 150 02

## Removal of peripheral boards from the system

In case of peripheral boards which are no longer used in the current configuration, the following procedure has to be performed in order to remove these boards from the system.

1. Switch off the system and remove the desired boards from the cabinet.
2. Switch on the system again (The system starts up and performs an automatic restart).
3. Connect BMS to the system.
4. Select ’Boards’ in the tree view to open the context menu
5. Click on “Hardware details” , the desired boards are shown as missing
6. Mark the desired board position and click on the ’Update’ button to remove the board.

Revision: T © Ericsson Enterprise 2005