BusinessPhone Communication Platform 7.0
Commands > Commands 0000...0999

## 0178
CallList allowed?

This command defines if a specified extension is allowed to have a call list or not.

##### Valid data

0 |  | no call list (default) |
1 |  | public incoming unanswered calls |
2 |  | public incoming answered calls |
3 |  | public incoming unanswered + answered calls |
4 |  | all public outgoing calls |
5 |  | public incoming unanswered + all public outgoing calls |
6 |  | public incoming answered calls + all public outgoing calls |
7 |  | public incoming unanswered calls + public incoming answered calls + all public outgoing calls |
8 |  | all internal calls |
9 |  | public incoming unanswered calls + all internal calls |
10 |  | public incoming answered calls + all internal calls |
11 |  | public incoming unanswered + answered calls + all internal calls |
12 |  | all public outgoing calls + all internal calls |
13 |  | public incoming unanswered + all public outgoing calls + all internal calls |
14 |  | public incoming answered calls + all public outgoing calls + all internal calls |
15 |  | public incoming unanswered calls + public incoming answered calls + all public outgoing calls + all internal calls |

Note

The value is needed for script programming

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005