BusinessPhone Communication Platform 7.0
Commands > Commands 9000...9999

## 9121
NPI for private/public called number 2

TThe command is used to define the Number Plan Identifier (Number Plan and Type Of Number) of the called number.

Following combinations of NPI's, Number Plan / Type Of Number, are available for the private network (CN) calls:

value | Number Plan | Type Of Number
00h | Public | Unknown
01h | Public | International
02h | Public | National
04h | Public | Subscriber
10h (default) | Private | Unknown
12h | Private | Regional level 1
14h | Private | Regional level 0 (local)
20h | Unknown | Unknown *

- * Used e.g. when characters * and # are send as digit-information in a number

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005