BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1032
Trunk impedance adaption

The command is used to state whether or not the automatic trunk impedance adaption (ATIA) has to be used. At transit calls ATIA is controlled by an additional parameter (command 1033 Impedance adaption for transit calls).

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005