BusinessPhone Communication Platform 7.0
Facilities

## Save/Redial for Incoming Calls

## Definition

Save or redial for incoming calls means that a incoming A-number can be saved (stored) in a memory by pressing the Save/Redial button on the telephone.

When the extension is in idle state, the saved number can be redialed by pressing the Save/Redial button on the telephone.

## Use

The feature enables the user to save and redial an
A-number of an incoming call in speech state for the purpose of dialing the number at a later time.

The A-number of the incoming call will be stored as soon as the user presses the menu key or the programmable key for saving the number in their own predefined memory position.

If you want to redial the number, press the Save/Redial button and the number will be automatically dialed.

## Operation

### DBC 210 and DBC 199 Telephones

Save number

An extension saves a dialled number as follows:

1. Press pre-programmed Save/Redial-key during a call attempt or during a call.

- Key depression does not affect ongoing calls or conversations.

#### To retransmit saved number

1. Press pre-programmed Save/Redial-key when telephone is idle.

- System seizes Line 1 or Inquiry and then selects free trunk by sending stored digits.

### DBC 220, DBC 211, DBC 222, DBC 212 and DBC 631 Telephones

#### Save number

An extension saves a incoming number as follows:

1. Press 2nd-key.
2. Press fixed key Save/Redial or pre-progammed key Save/Redial during a call attempt or during a call.

- Key depression does not affect ongoing calls or conversations.

#### To retransmit saved number

1. Press 2nd-key.
2. Press fixed key Save/Redial or pre-progammed key Save/Redial when telephone is idle.

- System seizes Line 1, Line 2 or Inquiry and then selects free trunk by stored digits can be sent.

A telephone with display shows the transmitted digits.

### DBC 223, DBC 213 and DBC 662 Telephones

#### Save number

- On the DBC 223, DBC 213 and DBC 662 telephones the are
  3 possibilities to save the incoming number:

- Using softkey
- Using fixed key Save/Redial
- Using programmable key Save/Redial

An extension saves an incoming number as follows:

1. Press Menu-key Save (see display) during a call attempt or during a call.

- Key depression does not affect ongoing calls or conversations

#### To retransmit saved number

1. Press Menu-key Redial (see display) when telephone is idle.

- System seizes Line 1, Line 2 or Inquiry and then selects free trunk by stored digits can be sent.

The display shows the transmitted digits.

## Capacity

Each extension can save one external number with a maximum of 24 digits including intermediate tone(s)
(if any) and area code.

## Limitations

The feature Save/Redial for Incoming Calls is not available for DBC 224, DBC 214 and DBC 663 telephones.

All other limitations are the same as for the existing feature Save External Number Redial Limitations.

## Programming

0301 |  | Key function

Enter function code = 37

## Equipment

System Telephones

Revision: F © Ericsson Enterprise 2005