BusinessPhone Communication Platform 7.0
Dialogs

## Private Network Router -Parameters

Facilities of this type can be created, deleted, or altered using the standard facility management dialog.

To access the dialog, open the “Facilities” menu in the Configuration directory tree. Then open the “Networking” submenu and click on “Private Network Router”. The Edit/Change section shows all private network routers that have been created. Click on a Parameters link of a router to open the parameters dialog.

In the first section, you can set the directory number and name. The second section is called “General”. Here you can make the following settings:

9101 |  | Destination PBX

9102 |  | Call back allowed?

9103 |  | NPI for private calling/connected line identification

9104 |  | Call class

9105 |  | NPI for public calling/connected line identification

9110 |  | 1st-route choice

9111 |  | NPI for private/public called number 1

9112 |  | Remove digits choice 1

9113 |  | Predigits choice 1

9114 |  | Travelling Class Mark 1

9115 |  | Complete called party NL 1

9116 |  | Subscriber called party NL 1

9117 |  | Node reference 1

9120 |  | 2nd-route choice

9121 |  | NPI for private/public called number 2

9122 |  | Remove digits choice 2

9123 |  | Predigits choice 2

9124 |  | Travelling Class Mark 2

9125 |  | Complete called party NL 2

9126 |  | Subscriber called party NL 2

9127 |  | Node reference 2

9128 |  | Send expensive route warning tone 2

9130 |  | 3-rd route choice

9131 |  | NPI for private/public called number 3

9132 |  | Remove digits choice 3

9133 |  | Predigits choice 3

9134 |  | Travelling Class Mark 3

9135 |  | Complete called party NL 3

9136 |  | Subscriber called party NL 3

9137 |  | Node reference 3

9138 |  | Send expensive route warning tone 3

9140 |  | 4-th route choice

9141 |  | NPI for private/public called number 4

9142 |  | Remove digits choice 4

9143 |  | Predigits choice 4

9144 |  | Travelling Class Mark 4

9145 |  | Complete called party NL 4

9146 |  | Subscriber called party NL 4

9147 |  | Node reference 4

9148 |  | Send expensive route warning tone 4

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To reload the current system settings. |
Copy |  | To copy the current settings to another router. |
Back |  | To return to the previous dialog. |

See Facility Descriptions:

- Networking – Based On Analogue Lines
  (361/15534-ASB 150 02 Uen).
- Networking – VPN Service From PSTN
  (364/15534-ASB 150 02 Uen).
- Networking – Based On Digital Lines
  (365/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2005