BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1303
Impulse type

The command is used at impulsing to determine the dialed digit’s relation to the number of pulses.

The number of impulses 1 2 3 4 5 6 7 8 9 10

0 = digit 1 2 3 4 5 6 7 8 9 0 |  |

1 = digit 0 1 2 3 4 5 6 7 8 9 |  |

2 = digit 9 8 7 6 5 4 3 2 1 0 |  |

3 = digit 0 9 8 7 6 5 4 3 2 1 |  |

Value = 0-3

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005