BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2146
GW Network access

For each of the in command 2145 GW RAS transport address defined GWs it has to be specified if the GW is accessible only within the system where it resides (with other words: accessible from all GWs that are registered to the same GK) or if it is also accessible from other systems (located via LRQ - Location ReQuest - procedure)

##### Valid data

0 |  | local (default) |
1 |  | local and network |

Note

Seen from this command:
Users of “strange” gateways (gateways, that are registered at any other GK) can use the “local‑GW” by dialling e.g. the LOC of the “GK‑node” and the PNR (or route or trunk individual number) to the “local‑GW” - in this case the “GK‑node” acts as a transit node, which means that 2 IP‑channels of the “GK‑node” are occupied.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005