BusinessPhone Communication Platform 7.0
Commands > Commands 3000...3999

## 3503
PBX queue announcement reference

This command defines the reference number of the queue announcement for a PBX group from a specific announcement group, dedicated for PBX group voice prompts.

The announcement will be played, if a call is queued in a PBX group because of all members are busy.

The voice prompt will be started after a certain delay (see also command 3504).

The given reference (vv) is supposed to have been recorded according to command 4436.

Note that recording in command 4436 is only possible on a VMU-HD or MFU board.

##### Valid data

0-15 |  |  |
-- |  | (default) (For no reference number the sending of a queue announcement will be disabled) |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005