BusinessPhone Communication Platform 7.0
Commands > Commands 8000...8999

## 8415
Arranging number to send

This command allows you to determine for the carrier how the number should be sent. Up to 8 number components can be specified for arranging. The specified components will be sent in the order as defined by the position number.

Parameters can be programmed only for: Delay time (0-30 seconds)

Available number components: B-number, External access code, Authority code, Account code, Own extension number, Change to DTMF, Wait on proceed-tone (see command 1314 Type of dial tone receiver, TRC), Delay time (0-30 seconds)

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005