BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2194
H.323 Trunk GW Q.931-port

Defines the Q.931‑port of the H.323 Trunk Gateway. The H.323 Trunk GW Q.931‑port must have a different value as command 2185 H.323 Extension GW Q.931-port. If modified, a restart of the IPU is required.

If modified, a restart of the IPU is required.

##### Valid data

0-65535 |
10040 (default) |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005