BusinessPhone Communication Platform 7.0
Commands > Commands 4000...4999

## 4902
Number of external lines

This command is used to state the maximum number of external lines permitted in a conference. The number includes connections with the public exchange and other PABX(s).

Range of values = 1-5

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005