BusinessPhone Communication Platform 7.0
Warning Messages ASB 150 02 >

## 0x37
Message To Non-Installed Card/Individual

Default definition: |  | ERROR + TRIG |
Used by block: |  | ALL |
Category: |  | DESIGNER |

A message has been received to a card or individual that is not correctly initiated. The EEPROM data is not valid or there has not been sufficient RAM available.

- D1: Received card position
- D2: Received INFCODE
- D3: Received SUBCODE
- D4: Received DATA+1

If ‘OS.WARNING code,DY’ is not used, data D3 and D4 are supplied by OS from the ME-register.

Revision: K © Ericsson Enterprise 2005