BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1036
Type of IBERCOM network connection

This command is used to define the type of ‘call class’ for some market specific traffic cases.

In case of Spanish market the external call setup for this call destination can be defined as an IBERCOM call with related parameters. The used network protocol on the actual (T-) link must be set to ‘network acc. to Spain’.

#### Additional function - independent on the used network protocol - since release 13 R8A or release 14 R2A:

If the command is set to IBERCOM network connection (value 1 or 3) the diverting number is used for A-number sending in case of external diverted and internal originated calls.

Note

The PNR command 9104 Call class overrides the trunk 1036 command.

##### Valid data

Value = |  | 0 |  | not specified (no IBERCOM network connection) (initial value) |
|  | 1 |  | interuser IBERCOM network connection |
|  | 3 |  | intrauser IBERCOM network connection |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005