BusinessPhone Communication Platform 7.0
Warning Messages ASB 150 02 >

## 0xE4
RP IPU Alarm

Default definition: |  | ALARM + EXTERN + ACTIVE + TRIG |
Used by block: |  | IPU |
Category: |  | DESIGNER |

Intermediate IPU warning level.

A severe fault has been detected by the IPU software. Immediate attention and user assistance is required.

- D1: Originating IPU software block, high byte
- D2: Originating IPU software block, low byte
- D3: Details on the fault reason, high byte
- D4: Details on the fault reason, low byte

Revision: K © Ericsson Enterprise 2005