BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2189
NPI aliases for called number - incoming

The command “Number Plan Identifier (Number Plan and Type Of Number) aliases for called number - incoming” defines a table of 30 NPI aliases with which the GW - GateWay registers to the GK - GateKeeper. Each of them consists out of up to 16 digits and a corresponding type of number value.

When programming this table the user gets an additional frame showing all the configured PNR codes with a possibility to simply pick an entry and enter it in the GW alias table. Nevertheless, such entries can be changed manually without influencing the actual PNR programming.

Whenever deleting or changing PNR entries (in an IPU equipped system) the BMS issues a warning pointing out possible data inconsistence in the GW alias table - e.g. a GW is registered for calls to a TDM (Time Division Multiplexing) node represented by a PNR entry which has been deleted.

##### Valid data per H.323 trunk GateWay:

| Type of Number | Number information
1-30 | 00-10 | 0-16 digits
1-30 | 0 (default) | empty (default)

##### Valid data for Type of Number:

value | Number Plan | Type Of Number
00h (default) | Public | Unknown
01h | Public | International
02h | Public | National
03h | Public | Network specific
04h | Public | Subscriber
06h | Public | Abbreviated
08h | Private | Unknown
09h | Private | Regional level 2
0Ah | Private | Regional level 1
0Bh | Private | Network specific
0Ch | Private | Regional level 0 (local)
0Eh | Private | Abbreviated
10h | Unknown | Unknown

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005