BusinessPhone Communication Platform 7.0
Commands > Commands 0000...0999

## 0195
CPN modification at call from ME?

The command is used to state whether a number modification of the inband received Called Party Number (CPN) at call from Mobile Extension (ME) is possible.

In order to prevent a delayed call setup to the wanted destination it is highly recommended to append to the CPN a ’#’ as ’forward-end-of-selection’ sign, either by programming the confirmation (verification) code to ’#’ (calling card functionality of mobile phone), or by dialling manually as additional digit. Otherwise call setups to the wanted parties are delayed according the timesupervison for digit receiving at incoming calls (command 1412 Time supervision between digits at automatic incoming traffic, default value 8 seconds).

All public called party numbers (CPN’s), that are used at calls from ME, must be stored in the phones directory book in a uniform way as international numbers (E.164). Public CPN’s must not have route access codes included, independent if the calls are established by utilizing the phone book, or by dialling manually. All internal CPN’s, used at calls from ME, can be stored in a the same uniform way as public CPN’s (e.g. +43 1 81100 1234) or just as internal directory number (e.g. 1234)

Limitation:The wanted public destination cannot be reached in case of short public CPN’s, with less or equal 4 digits, depending on the command xxxx

##### Valid data

0 |  | No |  | (default) |
1 |  | Yes |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005