BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1706
Seizure acknowledge

The command is used to state whether the signal “seizure acknowledge” shall be sent as reply to “seizure” at an incoming call.

Note

Ascertain whether the signal is included in the selected line signal scheme.

Value: YES or NO

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005