BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2092
Trunk route selected as PSTN-VPN call

The command states which trunk/route number shall be selected at VPN calls. The total number for accessing the network is assembled from the programmed trunk/route number (this command), the programmed predigits (command 2091 Predigits sent to PSTN-VPN) and the dialled number.

Example:

Dialled digits |  | 4711 |
Programmed trunk/route number |  | 88 |
Programmed predigits |  | 52304 |
Number for network access: |  | 88 52304 4711 |

Default data: EMPTY

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005