BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2181
H.323 Extension GK IP-address

Defines the IP-address of the Gatekeeper to which the Gateway for H.323 clients has to register

##### Valid data

0.0.0.0 - 255.255.255.255:(0 - 65535) |  |  |
0.0.0.0 (default) |  |  |

Note

The IP-address must be equal to the value of command 2152 IP address (own) of the IPU on which the Gatekeeper is activated

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005