BusinessPhone Communication Platform 7.0
Commands > Commands 6000...6999

## 6805
Tenant/Subscriber code

This command defines the subscriber code for a given tenant group in conjunction with the feature ’Inband CPN’ for Mobile Extensions. The complete own system id. (identification) is composed of own Country Code + Area Code + SUBScriber code number parts in according to E.164 number plan.

The programmed own system id. is compared with the received called party digits whereby a number translation is accomplished for a proper call setup to desired destination.

#### Prerequisites for number translation

A received called number from Mobile Extension, defined as ’Inband CPN’, is identified by the system as either ’own internal call destination’ or ’other external call destination’. This requires identification of own system which is done by programming of own complete public number, e.g.:
Own country code, command 2236: 43
Own area code,command 2237: 1
Own subscriber code, command 6805: 81100
This gives own system public number id.: 43181100

An external call destination may be prefixed, depending of the destination, e.g.:
International prefix, command 1936: 00
National prefix, command 1937: 0

An external routed call needs a route access definition, e.g.: Tenant route, command 6803: 00

Example 1: ME calls an internal destination with its own public number

The user dials with usage of phone book: (00) 43 1 81100 1234.
(00)431811001234: received digits
43181100 xxxx: own system id.
Probably leading prefix’s (00) are remove, thereafter are received digits compared to digit mask. Matching digits are removed, remaining digits are used for the new call setup, here:
1234: any internal dir. no.

Example 2: ME calls an local external destination

The user dials manually or using phone book: (00) 43 1 81200 4567
(00)431812004567: received digits
43181100 xxxx: own system id.
Probably leading prefix’s (00) are remove, thereafter are received digits compared to digit mask. Matching digits are removed, remaining digits are used for the new call setup, i.e. local call.
External (route) access code is included to the number for the new call setup, here:
00 812004567: route access dir. no. + send digits

##### Valid data

empty |  | (default) |
1-16 digits |  | empty |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005