BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1965
Call transfer via hook-on from TE’s

This command defines whether or not transfer via hook-on is allowed from S-bus terminals.
Depending of this command hook-on during an inquiry call will be handled as normal disconnection (transfer not allowed) or as call transfer (transfer allowed).

Note

This command do not have any influence on the ISDN call transfer version “ECT SS” (Explicit Call Transfer).

##### Valid data

No (default) |  | transfer via hook-on not allowed |
Yes |  | transfer via hook-on is allowed |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005