BusinessPhone Communication Platform 7.0
Dialogs

## Link Parameter

The displayed link parameters depend on the trunk type and interface type assignment.

To select a link for configuration, enter or select a link number in the navigation section on top of the dialog.

Command | Value
– | Link Number | Existing link number 5 digits (0-9)

Input parameters can be marked (selected) via corresponding check boxes if appropriate. These selected parameters are then considered when the user wants to copy link data to other destination links. The (Un)select commands check box on top of the page can be used to (un)select all of the link parameters.

– | (Un)select commands | Y/N (toggle)

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To reload the current system settings. |
Copy |  | To load the dialog for copying parameters to another link. |

See Facility Descriptions:

- Networking – Based On Digital Lines (365/15534-ASB 150 02 Uen).
- ISDN Facilities (268/15534-ASB 150 02 Uen).
- Trunk (486/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2005