BusinessPhone Communication Platform 7.0
Commands > Commands 0000...0999

## 0143
Line break time for ELU-A

Line break time for analog extension.

With this command you can state the duration of a line break for an analog extension.

##### Valid data

0 |  | (default) |
1-255 |  | ms |

The value zero indicates no line break.

The duration of a linebreak can vary from 1 * 50 ms to 255 * 50 ms.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005