BusinessPhone Communication Platform 7.0
Commands > Commands 4000...4999

## 4904
Number of participants for attenuation

This command is used to state the number of participants required for the connection of attenuation.

If no value is stated, there will be no attenuation, irrespective of the number of participants.

Attenuation is always connected if more than one trunk is connected to the conference, irrespective of the command.

Range of values = 3 - 6

Revision: E © Ericsson Enterprise 2005