BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1419
Minimum supervision time between ringsignals

The command is used to state the minimum time slot (pause time) between ringing signals and clearing of call.

The time is stated in seconds.

Value = 01-20 (1-20 s)

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005