BusinessPhone Communication Platform 7.0
Dialogs

## Tone Definition (non-repetitive)

For non-repetitive tones, the repetition column is not accessible.

Command | Value
Internal fragment | Value Range: 0-19 (15)
External fragment | Value Range: 0-19 (15)
Signal Time | Value Range: 0-16000 s (empty means continuous)
Pause time | Value Range: 0-16000 s (empty means continuous)

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To load the current system settings. |

See facility description Ring And Tone Signals (443/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2005